# Robot maintenance guide

## Enter interactive commands with robot

setupPath

[apRobot,robot] = ApStartRobotRealmode(1,1)

methods(robot) to see all the defined methods of the java object

## Trace to file or console

robot.SetTraceFileOn(1)

robot.SetTraceFileOn(0)

## To trace encoder et power data

robot.SetUdpTrace(0) >> trace off

robot.SetUdpTrace(1) >> trace on